Default FSX to P3Dv3/P3Dv4 Portover - DG808S
============================================

Just copy the folder DG808S from FSX to your P3D simobjects/aircraft folder.

Copy the texture.nzff folder into the DG808S folder, then edit the aircraft.cfg file to include the entry below (replacing "xx" with the next number in the sequence).

// ============================================================================

[fltsim.xx]
title=DG808S - NZFF
sim=DG808S
model=
panel=
sound=
texture=nzff
kb_checklists=DG808S_check
kb_reference=DG808S_ref
atc_id=ZK-NZF
ui_manufacturer="DG Flugzeugbau"
ui_type="DG-808S"
ui_variation="NZFF"
ui_typerole="Glider"
ui_createdby="Microsoft"
description="The DG-808S Competition is a lightweight, high-performance sailplane constructed with composite materials. It features a sophisticated water ballast system that allows the pilot to tailor wing loading to prevailing weather conditions. In weak thermals, the large surface area of the sailplane’s 59-foot (18-meter) wingspan makes for high lift and good climb performance without ballast.\nIn heavier weather, the DG-808S Competition’s combination of low weight and high strength allows it to take off at more than twice its empty weight with enough ballast to soar in strong thermals. In all conditions, its upswept winglets increase the sailplane’s already excellent glide ratio.\nFictional repaint by Adamski_NZ."

// ============================================================================

Note: In P3D, CTL-SHF-Y will bring up the deafualt Maule Orion as a tow plane. It will take off and keep climbing in a straight line from the current runway heading. SHF-Y disconnects. Needs a fair bit of down-trim on take off - or you'll break the wire!

Adamski.
02 July 2016
www.nzfsim.org